{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Darcy Forchheimer calculator"],"not_rendered":{"charts":1,"images":3,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Darcy Forchheimer calculator","index":0,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,0,1,2],[2,0,2,2],[9,0,10,0]]}
[{"$error":"#VALUE!"}]
[]
["Porocity coefficient calculator"]
[]
["Length [m]",1,null,"Air velocity [m/s] ","Pressure drop [Pa]"]
["Air density [kg/m3 ]",1.2250000000000001,null,1,36.265000000000001]
["Dynamic vicosity [Pa·s]",1.789E-5,null,5,548.82500000000005]
[null,null,null,10,2016.4]
[{"$error":"#VALUE!"},null,null,15,4402.7250000000004]
[{"$error":"#VALUE!"},null,null,20,7707.8]
[]
[]
["A",{"$f":"INDEX(LINEST(Tabell1[Pressure drop '[Pa']], Tabell1[Air velocity '[m/s'] ]^{1,2},FALSE), 1)","v":18.375}]
["B",{"$f":"INDEX(LINEST(Tabell1[Pressure drop '[Pa']], Tabell1[Air velocity '[m/s'] ]^{1,2},FALSE), 2)","v":17.89}]
["Darcy coefficient (D)",{"$f":"18.357/(B5*B7)","v":1026103.9686975963}]
["Forcheimer coefficient (F)",{"$f":"(2*17.89)/(B5*B6)","v":29.208163265306123}]
["R2",{"$f":"INDEX(LINEST(Tabell1[Pressure drop '[Pa']], Tabell1[Air velocity '[m/s'] ]^{1,2},FALSE,TRUE), 3, 1)","v":1}]